Next: Further Details: Floating Point Up: Accuracy and Stability Previous: Accuracy and Stability Contents Index

#
Sources of Error in Numerical Calculations

There are two sources of error whose effects can be measured by the bounds in this chapter: roundoff error and input error. Roundoff error arises from rounding results of floating-point operations during the algorithm. Input error is error in the input to the algorithm from prior calculations or measurements. We describe roundoff error first, and then input error.

Almost all the error bounds LAPACK provides are multiples of machine epsilon, which we abbreviate by . Machine epsilon bounds the roundoff in individual floating-point operations. It may be loosely defined as the largest relative error in any floating-point operation that neither overflows nor underflows. (Overflow means the result is too large to represent accurately, and underflow means the result is too small to represent accurately.) Machine epsilon is available either by the function call SLAMCH('Epsilon') (or simply SLAMCH('E')) in single precision, or by the function call DLAMCH('Epsilon') (or DLAMCH('E')) in double precision. See section 4.1.1 and Table 4.1 for a discussion of common values of machine epsilon.

Since underflow is almost always less significant than roundoff, we will not consider it further. Overflow usually means the computation is invalid, but there are some LAPACK routines that routinely generate and handle overflows using the rules of IEEE arithmetic (see section 4.1.1).

Bounds on input errors, or errors in the input parameters inherited from prior computations or measurements, may be easily incorporated into most LAPACK error bounds. Suppose the input data is accurate to, say, 5 decimal digits (we discuss exactly what this means in section 4.2). Then one simply replaces by in the error bounds.

- Further Details: Floating Point Arithmetic

Next: Further Details: Floating Point Up: Accuracy and Stability Previous: Accuracy and Stability Contents Index